**Satellite Signal Finder**

* For use to peak up an antenna on a satellite
* Features a variable tone to indicate power level for a satellite
* RF and DC Pass Through
* Frequency 950 ~ 2150MHz
* Front panel sensitivity control